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NBS SPECIFICATION
N10 General Fixtures/Furnishings/Equipment
Laminate Worktop with Integral Coved Upstand
	PROJECT
[Insert project name]
	PREPARED FOR
[Architect / Contractor]
	DATE
November 2026
	REVISION / STATUS
A — For Approval


200   WORKTOPS — LAMINATE WITH COVED UPSTAND
	Location
	Refer to Architect's drawings.

	Manufacturer
	Bridgewater Direct, Unit 1C Britannia Business Park, Union Road, Bolton BL2 2HP. Tel: 0161 703 3980 · sales@bridgewaterdirect.co.uk · www.bridgewaterdirect.co.uk

	Product reference
	Laminate Worktop with Integral Coved Upstand — 40 mm core, 75 mm coved upstand

	Construction
	40 mm chipboard core faced in non-porous, wipe-clean high-pressure laminate (HPL).

	Rear upstand
	75 mm integral coved upstand, formed in one piece with the worktop surface, with no seam at the back edge. 115 mm overall height.

	Front edge & ends
	Postformed front edge. Both ends capped.

	Size, to the millimetre
	Width 400–2900 mm, wall to wall. Depth 400–900 mm, including the upstand.

	Cut-outs & joints
	Sink cut-outs, tap holes, joints and non-standard layouts quoted from the project drawing.

	HTM 63 status
	Not supplied as an HTM 63 product and carries no hygiene certification. Where the specification names HTM 63, use the Bridgewater Direct HTM 63 Laminate Worktop.

	Colour (Architect to select)
	BD White, BD Dove Grey, BD Graphite, BD Natural Oak, BD Pearl Stone or BD Slate Stone.
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Section through the worktop, 600 mm depth shown. Upstand thickness and radii are indicative: refer to the manufacturer.
INSTALLATION
1. Programming: Do not install until the building is weathertight and dried out and wet trades have finished.
1. Measuring: Wall to wall at the back, then front to back at the deepest point. Confirm before manufacture.
1. Modifications: Do not cut, plane or sand prefinished components. Seal all edges of any opening cut on site.
1. Fixing by others: Secure to the supporting units or framework and seal the upstand to the wall.
1. Moisture and movement: Make adequate allowance for future movement.
SAMPLES & TECHNICAL SUPPORT
Decor samples, datasheets and project advice are available direct from Bridgewater Direct: call 0161 703 3980 or email sales@bridgewaterdirect.co.uk quoting the product reference above, or configure online at www.bridgewaterdirect.co.uk.
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